**Installation Check List**

* Has Gauge(s) been installed
* Are filters in place and sealed
* Has sight been cleaned up and all debris removed
* Has Field report been filled out and signed by customer
* Has control panel(s) been secured to collector
* Are duct runs verified to be level
* Are seams on duct facing the ceiling and not visible from ground level
* Are slip tube connections facing in proper direction relative to air flow
* Has owner manual been delivered to customer
* At start up is fan rotation correct