Wake Tech Punchlist / 1-25-11

The following items need to be checked out / fixed on every booth:

1. Make sure the pins are tapped into the hinges on the clean out door.

There are 3 hinges per door.

1. On booth number 20: Fill the screw holes from the hinge with two screws
2. On booths 3 and 13: Flatten out the flange on the control box and bolt back to the unit. Check all booths again.
3. Make sure all floor levelers are touching the floor.
4. Install two lights on booths 13 and 14.
5. On all booths tie up the cord from the lights. Use zip ties to wrap around the bolt.
6. Check all booths for scratches and paint. Check ceilings, front side, edges, all areas of the booths.
7. Control Panel: Tighten conduit going into the box and straighten all labels.