# SDC-AT-3-12 specs

**12 Horizontal Cartridge Collection System**

* 12 Horizontal cartridge down-flow dust collector
* Holds 12 filter cartridges totaling 3,048 sq ft of filter media
* Nano fiber Merv 15 filters
* Pulse control timer board with built in digital pressure gauge
* Goyen solenoid diaphragm valves
* Drum lid
* Quick lock easy access door
* Heavy duty 7 and 10 gauge steel construction
* 5 year warranty
* Made in USA
* TCBI 15 HP motor with direct drive top mount opposed blade fan.
* 5,000CFM at 12”
* Dam 30 Damper for TCBI 15.
* In line spark trap with access door.
* Drum latch for 55 gallon drum (drum not included).
* 15HP all in one starter/disconnector/pulse timer board with digital pressure gauge

